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General Items to be completed:
|_| All Drawing notes are accounted for on AS9102C Form 3
|_| All Quality Requirements are accounted for on AS9102C Form 3
|_| Reviewed Supplier Policy Manual for any additional quality requirements (labels for cable assemblies, IPC requirements, etc.) – List Supplier Policy Manual on AS9102C Form 3 (This is attribute data, accept or reject)
|_| All dimensions are accounted for on the AS9102C Form 3, results are recorded and within specification.
|_| A ballooned/bubbled drawing has been provided when there are more than 20 reportable dimensions.
|_| If a dimensioned drawing was not provided by PZ a vendor supplied drawing is included.
|_| Certifications (COC) for any referenced materials or special processes on the drawing or parts list have been provided.
|_| Certifications (COC) for any commercial parts identified on the drawing or parts list have been provided.
|_| If there are lower level parts manufactured to a PZ drawing a separate FAI has been provided for these.
|_| Non-conformances have been identified and approved in advance of shipment.
|_| Deviation/Waivers have been identified and approved in advance of shipment
|_| Documentation package has been provided with the shipment of the FAI part or sent electronically (preferred method) to the buyer or supplier quality at the time of shipment.
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